**Water Supply Program on COVID-19 during Worst Situation.**

**Overall Incharge for water: Mani Kumar Rizal, Engineer (17661316)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl No** | **Coverage** | **Present Situation** | **During worst situation** | **Remarks** |
| 1 | Core Town, SJ | Bore well water routine supply | * Police supply hours shall drop by two hrs and same water shall provide to Town. * Additional Supply through Tanker shall be provided at the quarantine place (hotels) | Firoz Rahiman, 77671490.  Location of Resident: Lower market near STP. |
| 2 | LAP2,3,4 (above Dungsum bridge, all) Dzong area, Royal Guest House | Normal supply from WTP at Pinchinang | * The Supply shall be done to the storage Tank above guest house and shall supply to the consumer as per schedule. * The fire Hydrant tank above Dechen pry school shall operate for tanker supply as well to the consumer. * The Hospital storage tank near Zangdopelri shall be utilised as additional top up to Hospital. (Hospital ADM shall manage) | Tshering Dorji, 17838299,  Location of Resident: near Dzong canteen**.** |
| 3 | For whole Samdrupjongkhar | WTP functioning on manual mode | * Out of 4, 2 numbers of our staff shall be withdrawn from WTP operation and shall deputed patrolling for any break down of supply line (both gravity and pump line). * Backup Supply from infiltration gallery shall operate. * Project operating staff shall also be engaged. | BimalSubba17388772, Sonam Choeda 77670686, Tashi Wangchuk 77357155, Sangay penjor 77665912.  Dawa (project Staff) :77879074 |
| 4 | Throm | None | * SMCL, RBP Tankers shall be requested for supply in the quarantine centers if necessary | GM (17114561) |
| 5 | Deothang area | Supply from three water sources: Lemsonrong at 18Km away, Zalakhee at 2Km away and Gaykheree within thromde area) | * The Supply shall be 24 hrs. Three plumbers recruited on Muster roll are on duty. | Sonam Drupchu 77666304.  Sherub Wangdi 17977631  Bal Bdr Tamang 77346115 |

**Back up plan for water supply**

**Additional infiltration gallery is constructed and pumps are on standby in case of failure of WTP.**

**Restoration of old pump gallery will be completed 21/4/2020 where seepage water from the river will join with WTP.**

**3 numbers of water tanker including one from SMCL available (Drivers Nar Bdr 16925424), Kamal 17945183)**

**Additional pumps as a backup stock being ordered and will reach SJ before end of April 2020.**

**Sanitation part.**

**Sewerage block clean and septic tank clearing by suction tank (Pasang 17678711)**

**Garbage collection will be normal (In charge Sonam Choden 17504282)**

**Deputed Tractor for collection of waste from quarantine centers and isolation ward. Incineration of such waste will be done by BAFRA supported by Thromde. (Tractor Driver 17948539)**